|  |  |  |  |
| --- | --- | --- | --- |
| 1 | 6 | Kit | Packing kit for triplex bomb 3”. Part number: 2A140373 |
| 2 | 50 | Piece | 1502 Weco Seals in Viton material MCA. FMC |
| 3 | 20 | Kit | Packing kit for Chiksan 2”. MCA. FMC. Part number: P554011 |

|  |
| --- |
| Description |
| Stripper rubber for TF of ¾. TOT Part number: 8412-6044 |
| 3” Suction Valve. Part number: 07124684RD |
| 3” Discharge valve. Part number: 071240683 or Part Number: 2-WG-3 |
| Seat with Oring per triplex bomb valve of 3”. Part number: 01559475 |
| Counter balance HR680 Part Number: HVP00298 |

|  |  |  |
| --- | --- | --- |
| Quantity | Unity | Material description |
| 1 | Piece | Expansion gate valve of 2 1/16” 5M PSI, Flanged ends API 6A LU, DD, PSL 1, PR1 (010-95885) |
| 1 | Piece | Expansion gate valve of 2 9/16” 5M PSI, Flanged ends API 6A LU, DD, PSL 2, PR1 (010-96885) |
| 1 | Piece | Expansion gate valve of 3 1/8” 5M PSI, Flanged ends API 6A LU, DD, PSL 1, PR1 (010-96885) |
| 1 | Piece | Expansion gate valve of 4 1/16” 5M PSI, Flanged ends API 6A LU, DD, PSL 2, PR1 (010-JM108) |
| 1 | Piece | Cross of 2 1/16” 5M PSI X 2 1/16” 5M PSI X 2 1/16” 5M PSI X 2 1/16” 5M PSI, LI, DD, PSL-2, PR1 (14-02525) |
| 1 | Piece | Cross of 2 9/16” 5M PSI X 2 9/16” 5M PSI X 2 1/16” 5M PSI X 2 1/16” 5M PSI, LI, DD, PSL-2, PR1 (14-02505) |
| 1 | Piece | Cross of 3 1/8” 5M PSI X 3 1/8” 5M PSI X 2 1/16” 5M PSI X 2 1/16” 5M PSI, LI, DD, PSL-2, PR1 |
| 1 | Piece | Background test adapter (Hat) of 2 1/16” 5M PSI X 2 3/8” EUE LU, DD, PSL-2, PR1 (06-09200-M) |
| 1 | Piece | Background test adapter (Hat) of 2 9/16” 5M PSI X 2 7/8” EUE LU, DD, PSL-3, PR1 (006-09250-M) |
| 1 | Piece | Background test adapter (Hat) of 3 1/8” 5M PSI X 3 1/2” EUE LU, DD, PSL-3, PR1 |
| 1 | Piece | Background test adapter (Hat) of 4 1/16” 5M PSI X 4 1/2” EUE LU, DD, PSL-1, PR1 (006-09400) |
| 1 | Piece | Positive choke holder of 2 1/16” 5M PSI, Flanged ends, LU, EE, PSL-2, PR1 (016-02241) |
| 1 | Piece | Positive choke holder of 2 9/16” 5M PSI LU, DD, PSL-2, PR1 |
| 1 | Piece | Solid gate valve of 2 1/16” 10M PSI, Flanged ends, API 6A LU, EE, PSL-3, PR1 (10-FC003) |
|  | Piece | Solid gate valve of 3 1/8” 5M PSI, Flanged ends, API 6A LU, DD, PSL-2, PR1 (10-FC006) |
| 1 | Piece | Solid gate valve of 3 1/16” 10M PSI, Flanged ends, API 6A LU, EE, PSL-3, PR1 (10-FC007) |